Set-Point, Ysp Controller

Signal from sensor, Y

Error, E + -

Signal to actuator, U